<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="150" y2="0" width="0" layer="20"/>
<wire x1="150" y1="0" x2="150" y2="100" width="0" layer="20"/>
<wire x1="150" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text>Eclaire XL
(c)2016
Mark Watson
V1.3</text>
<text>AUDIO</text>
<text>8-bit
V DAC</text>
<text>10-bit
 A/D </text>
<text>V G A</text>
<text>TEST POINTS!!</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="L3225M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="DIL-100-2X05-BRD">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SG-636">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB15">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="Analog Devices_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 31/07/2012 09:37:13</description>
<packages>
<package name="QFP50P900X900X120-49N">
</package>
</packages>
</library>
<library name="con-usb-3">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Erik Christiansson (erik@alphafish.com)&lt;/author&gt;&lt;p&gt;
Based on the datasheets for the following products.&lt;br&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;Manufacturer&lt;/td&gt;&lt;td&gt;Part No.&lt;/td&gt;&lt;td&gt;Type&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04AFDXX0&lt;/td&gt;&lt;td&gt;Series A Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04AFHSW0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C3817-04AFVSW0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted Up-Right&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04BFHSW0&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8320-05BFDSB0&lt;/td&gt;&lt;td&gt;Series Mini-B Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8320-05BFRSB0&lt;/td&gt;&lt;td&gt;Series Mini-B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Amp&lt;/td&gt;&lt;td&gt;787616-*&lt;/td&gt;&lt;td&gt;Series A Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Amp&lt;/td&gt;&lt;td&gt;787780-1&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;ACON&lt;/td&gt;&lt;td&gt;UAR80-4****0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted Up-Right&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;ACON&lt;/td&gt;&lt;td&gt;MNC20-5K5*1*&lt;/td&gt;&lt;td&gt;Series Mini-B Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Molex&lt;/td&gt;&lt;td&gt;67068-****&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-H">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="HALFHEIGHTSD">
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
</packages>
</library>
<library name="con-yamaichi">
<description>&lt;b&gt;Yamaichi Connectors&lt;/b&gt;&lt;p&gt;
Mini-DIN, USB, Fire Wire&lt;br&gt;
DIN female/male, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MDIN06SS">
<description>&lt;b&gt;Mini Din&lt;/b&gt; YAMAICHI CONNECTOR</description>
</package>
<package name="MDIN04SS">
<description>&lt;b&gt;Mini Din&lt;/b&gt; YAMAICHI CONNECTOR</description>
</package>
</packages>
</library>
<library name="de1_parts">
<packages>
<package name="DIL-100-2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 0.1"</description>
</package>
</packages>
</library>
<library name="resistor-array">
<description>&lt;b&gt;SMD Resistor Arrays&lt;/b&gt;&lt;p&gt;
CTS, Rohm, etc&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="743-8">
<description>CTS 744 Series&lt;p&gt;
8 Terminations, 4 Resistors</description>
</package>
</packages>
</library>
<library name="sdram">
<description>&lt;b&gt;SDRAM  memories&lt;/b&gt;

by Martin Hinner&lt;br&gt;
&lt;a href="http://martin.hinner.info/"&gt;http://martin.hinner.info/&lt;/a&gt;</description>
<packages>
<package name="TSOP54">
<description>TSOP 54 Pin, pitch 0.8 mm</description>
</package>
</packages>
</library>
<library name="Exar_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:16:13</description>
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
<library name="cyclonev_f484">
<packages>
<package name="CYCLONEVF484V2">
</package>
</packages>
</library>
<library name="Eagle_Wuerth_Elektronik_Switch_rev15b">
<description>&lt;BR&gt;Wurth Elektronik - Switches&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;WÃ¼rth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;WÃ¼rth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015b, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: WÃ¼rth Elektronik</description>
<packages>
<package name="ROCKER_VERT_SPDT2">
</package>
</packages>
</library>
<library name="adc">
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
<library name="j_usb_hirose_zx62d-b-5p8">
<packages>
<package name="ZX62D-B-5P8">
<description>Mounting pattern for Hirose ZX62D-B-5P8 Micro-B USB connector with SMD leads and through-hole shell connection. Modified from the manufacturer's recommendations by using round holes and leaving out shell SMD pads.</description>
</package>
</packages>
</library>
<library name="con-hirschmann">
<description>&lt;b&gt;Hirschmann Connectors&lt;/b&gt;&lt;p&gt;
Audio, scart, microphone, headphone&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TOBU3_EXT">
</package>
</packages>
</library>
<library name="Seeed-OPL-Switch">
<packages>
<package name="SW4-SMD-4.0X4.0X1.7MM">
</package>
</packages>
</library>
<library name="header127">
<packages>
<package name="HDR_141_36">
</package>
</packages>
</library>
<library name="epcs">
<packages>
<package name="EPCS_BOTH">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,5-PAD">
</package>
</packages>
</library>
<library name="raspberrypi_cm">
<packages>
<package name="HDMI">
</package>
</packages>
</library>
<library name="LIBstereoaudiojack">
<packages>
<package name="AUDIO-JACK-CUI-353X">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JTAG" library="con-headers-jp" package="DIL-100-2X05-BRD" value="M-2X05-BORDER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="M0805" value="1k-10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="M0805" value="1k-10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="M0805" value="2K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTL" library="crystal" package="SG-636" value="5MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="0.0047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VGA" library="SparkFun-Connectors" package="DB15" value="DB15">
<attribute name="VALUE"/>
</element>
<element name="VIDEODACSA" library="Analog Devices_By_element14_Batch_1" package="QFP50P900X900X120-49N" value="CDK3405">
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="M0805" value="348">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB.A" library="con-usb-3" package="USB-A-H" value="">
<attribute name="NAME"/>
</element>
<element name="USB.B" library="con-usb-3" package="USB-A-H" value="">
<attribute name="NAME"/>
</element>
<element name="R15" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="adafruit" package="HALFHEIGHTSD" value="SDMMCHALFHEIGHT"/>
<element name="R23" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PS/2" library="con-yamaichi" package="MDIN06SS" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="ZD1" library="adafruit" package="SOT23-R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ZD2" library="adafruit" package="SOT23-R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPIO_A" library="de1_parts" package="DIL-100-2X20" value="DE1_GPIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPIO_B" library="de1_parts" package="DIL-100-2X20" value="DE1_GPIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPIO_C" library="de1_parts" package="DIL-100-2X20" value="DE1_GPIO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN15" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDRAM" library="sdram" package="TSOP54" value="K4S561632E-TC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.3V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="3.3V">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2.5V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="2.5V">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1.1V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="1.1V">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="5V_IN_B" library="con-usb-3" package="USB-B-H" value="">
<attribute name="NAME"/>
</element>
<element name="U$1" library="cyclonev_f484" package="CYCLONEVF484V2" value="CYCLONEVFPGA484SMALLPINS"/>
<element name="C28" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0805" value="SP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0805" value="SP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0805" value="SP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER_SW" library="Eagle_Wuerth_Elektronik_Switch_rev15b" package="ROCKER_VERT_SPDT2" value="450302014072ROCKER2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PF1" library="rcl" package="R1206" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ADC" library="adc" package="SOT95P280X145-5N" value="MCP3021">
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C1206" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C1206" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-VIDEO" library="con-yamaichi" package="MDIN04SS" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="5V_IN" library="j_usb_hirose_zx62d-b-5p8" package="ZX62D-B-5P8" value="ZX62D-B-5P8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C-VIDEO" library="con-hirschmann" package="TOBU3_EXT" value="TOBU3MINE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="Seeed-OPL-Switch" package="SW4-SMD-4.0X4.0X1.7MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUDIO" library="LIBstereoaudiojack" package="AUDIO-JACK-CUI-353X" value="AUDIO-JACK2CUI"/>
<element name="C37" library="rcl" package="C0805" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="240">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN9" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN10" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN11" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN12" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN16" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN17" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN18" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN19" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="header127" package="HDR_141_36" value="HDR_SMALL_36_DEV_LALIGNED"/>
<element name="RN5" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN6" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN7" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN8" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN14" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN20" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN21" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN22" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN23" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="header127" package="HDR_141_36" value="HDR_SMALL_36_DEV_LALIGNED"/>
<element name="RN1" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN4" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN13" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN24" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN25" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN26" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN27" library="resistor-array" package="743-8" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="header127" package="HDR_141_36" value="HDR_SMALL_36_DEV_LALIGNED"/>
<element name="C38" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPI" library="epcs" package="EPCS_BOTH" value="EPCS">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="12T1359"/>
<attribute name="MPN" value="AT25320B-SSHL-B"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1841578"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.3/2.5/1.1/GND" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="M0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="M0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H2" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H3" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H4" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H5" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H6" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="H7" library="holes" package="2,5-PAD" value="MOUNT-PAD-ROUND2.5"/>
<element name="HDMI" library="raspberrypi_cm" package="HDMI" value="HDMI">
<attribute name="NAME"/>
</element>
<element name="RN28" library="resistor-array" package="743-8" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN29" library="resistor-array" package="743-8" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JTAG" pad="10"/>
<contactref element="JTAG" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="XTL" pad="P$2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="VIDEODACSA" pad="33"/>
<contactref element="VIDEODACSA" pad="31"/>
<contactref element="VIDEODACSA" pad="27"/>
<contactref element="VIDEODACSA" pad="1"/>
<contactref element="VIDEODACSA" pad="40"/>
<contactref element="VIDEODACSA" pad="39"/>
<contactref element="VIDEODACSA" pad="26"/>
<contactref element="VIDEODACSA" pad="25"/>
<contactref element="VIDEODACSA" pad="15"/>
<contactref element="VIDEODACSA" pad="14"/>
<contactref element="VIDEODACSA" pad="2"/>
<contactref element="VGA" pad="5"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="USB.B" pad="GND"/>
<contactref element="USB.A" pad="GND"/>
<contactref element="R20" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$2" pad="GP"/>
<contactref element="ZD2" pad="1"/>
<contactref element="PS/2" pad="3"/>
<contactref element="ZD1" pad="1"/>
<contactref element="GPIO_A" pad="12"/>
<contactref element="GPIO_A" pad="30"/>
<contactref element="GPIO_B" pad="12"/>
<contactref element="GPIO_B" pad="30"/>
<contactref element="GPIO_C" pad="12"/>
<contactref element="GPIO_C" pad="30"/>
<contactref element="GPIO_A" pad="12"/>
<contactref element="GPIO_A" pad="30"/>
<contactref element="GPIO_B" pad="12"/>
<contactref element="GPIO_B" pad="30"/>
<contactref element="GPIO_C" pad="12"/>
<contactref element="GPIO_C" pad="30"/>
<contactref element="SDRAM" pad="54"/>
<contactref element="SDRAM" pad="28"/>
<contactref element="SDRAM" pad="41"/>
<contactref element="SDRAM" pad="6"/>
<contactref element="SDRAM" pad="12"/>
<contactref element="SDRAM" pad="46"/>
<contactref element="SDRAM" pad="52"/>
<contactref element="1.1V" pad="2"/>
<contactref element="2.5V" pad="2"/>
<contactref element="3.3V" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="U$2" pad="GP3"/>
<contactref element="5V_IN_B" pad="GND"/>
<contactref element="VGA" pad="8"/>
<contactref element="VGA" pad="10"/>
<contactref element="VGA" pad="6"/>
<contactref element="VGA" pad="7"/>
<contactref element="VIDEODACSA" pad="12"/>
<contactref element="U$1" pad="B2"/>
<contactref element="U$1" pad="H4"/>
<contactref element="U$1" pad="M10"/>
<contactref element="U$1" pad="A21"/>
<contactref element="U$1" pad="T1"/>
<contactref element="U$1" pad="AB9"/>
<contactref element="U$1" pad="AB19"/>
<contactref element="U$1" pad="K1"/>
<contactref element="U$1" pad="F5"/>
<contactref element="U$1" pad="P10"/>
<contactref element="U$1" pad="R3"/>
<contactref element="U$1" pad="E3"/>
<contactref element="U$1" pad="P4"/>
<contactref element="U$1" pad="W4"/>
<contactref element="U$1" pad="N15"/>
<contactref element="U$1" pad="M2"/>
<contactref element="U$1" pad="M14"/>
<contactref element="U$1" pad="C17"/>
<contactref element="U$1" pad="H1"/>
<contactref element="U$1" pad="K2"/>
<contactref element="U$1" pad="L3"/>
<contactref element="U$1" pad="F16"/>
<contactref element="U$1" pad="AA4"/>
<contactref element="U$1" pad="E13"/>
<contactref element="U$1" pad="N13"/>
<contactref element="U$1" pad="N5"/>
<contactref element="U$1" pad="Y1"/>
<contactref element="U$1" pad="N17"/>
<contactref element="U$1" pad="L15"/>
<contactref element="U$1" pad="U5"/>
<contactref element="U$1" pad="L11"/>
<contactref element="U$1" pad="D10"/>
<contactref element="U$1" pad="L21"/>
<contactref element="U$1" pad="C4"/>
<contactref element="U$1" pad="H15"/>
<contactref element="U$1" pad="T2"/>
<contactref element="U$1" pad="Y18"/>
<contactref element="U$1" pad="E4"/>
<contactref element="U$1" pad="F2"/>
<contactref element="U$1" pad="M4"/>
<contactref element="U$1" pad="D1"/>
<contactref element="U$1" pad="M1"/>
<contactref element="U$1" pad="H7"/>
<contactref element="U$1" pad="V1"/>
<contactref element="U$1" pad="K12"/>
<contactref element="U$1" pad="C3"/>
<contactref element="U$1" pad="H12"/>
<contactref element="U$1" pad="K14"/>
<contactref element="U$1" pad="J3"/>
<contactref element="U$1" pad="B14"/>
<contactref element="U$1" pad="Y2"/>
<contactref element="U$1" pad="N11"/>
<contactref element="U$1" pad="F1"/>
<contactref element="U$1" pad="N3"/>
<contactref element="U$1" pad="W3"/>
<contactref element="U$1" pad="P2"/>
<contactref element="U$1" pad="V2"/>
<contactref element="U$1" pad="H3"/>
<contactref element="U$1" pad="H22"/>
<contactref element="U$1" pad="AB14"/>
<contactref element="U$1" pad="G9"/>
<contactref element="U$1" pad="R13"/>
<contactref element="U$1" pad="G4"/>
<contactref element="U$1" pad="V17"/>
<contactref element="U$1" pad="D2"/>
<contactref element="U$1" pad="U9"/>
<contactref element="U$1" pad="U4"/>
<contactref element="U$1" pad="V12"/>
<contactref element="U$1" pad="J20"/>
<contactref element="U$1" pad="AB2"/>
<contactref element="U$1" pad="K8"/>
<contactref element="U$1" pad="H2"/>
<contactref element="U$1" pad="G19"/>
<contactref element="U$1" pad="L5"/>
<contactref element="U$1" pad="B9"/>
<contactref element="U$1" pad="A11"/>
<contactref element="U$1" pad="U3"/>
<contactref element="U$1" pad="F6"/>
<contactref element="U$1" pad="AA6"/>
<contactref element="U$1" pad="J5"/>
<contactref element="U$1" pad="N7"/>
<contactref element="U$1" pad="P1"/>
<contactref element="U$1" pad="D5"/>
<contactref element="U$1" pad="V7"/>
<contactref element="U$1" pad="B1"/>
<contactref element="U$1" pad="K10"/>
<contactref element="U$1" pad="C5"/>
<contactref element="U$1" pad="AB1"/>
<contactref element="U$1" pad="K4"/>
<contactref element="U$1" pad="T16"/>
<contactref element="U$1" pad="F17"/>
<contactref element="U$1" pad="T21"/>
<contactref element="U$1" pad="J15"/>
<contactref element="U$1" pad="G3"/>
<contactref element="U$1" pad="AA11"/>
<contactref element="U$1" pad="Y5"/>
<contactref element="U$1" pad="D20"/>
<contactref element="U$1" pad="AA3"/>
<contactref element="U$1" pad="N22"/>
<contactref element="U$1" pad="V22"/>
<contactref element="U$1" pad="L13"/>
<contactref element="U$1" pad="V4"/>
<contactref element="U$1" pad="M12"/>
<contactref element="U$1" pad="A2"/>
<contactref element="U$1" pad="E5"/>
<contactref element="U$1" pad="G5"/>
<contactref element="C28" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="ADC" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C34" pad="1"/>
<contactref element="S-VIDEO" pad="1"/>
<contactref element="S-VIDEO" pad="2"/>
<contactref element="5V_IN" pad="P$5"/>
<contactref element="C-VIDEO" pad="2@1"/>
<contactref element="C-VIDEO" pad="2"/>
<contactref element="C-VIDEO" pad="2@2"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="AUDIO" pad="P$1"/>
<contactref element="R37" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="SPI" pad="4"/>
<contactref element="SPI" pad="L$10"/>
<contactref element="3.3/2.5/1.1/GND" pad="4"/>
<contactref element="C39" pad="2"/>
<contactref element="H5" pad="B2,8"/>
<contactref element="H3" pad="B2,8"/>
<contactref element="H1" pad="B2,8"/>
<contactref element="H2" pad="B2,8"/>
<contactref element="H4" pad="B2,8"/>
<contactref element="H6" pad="B2,8"/>
<contactref element="H7" pad="B2,8"/>
<contactref element="HDMI" pad="2"/>
<contactref element="HDMI" pad="5"/>
<contactref element="HDMI" pad="8"/>
<contactref element="HDMI" pad="11"/>
<contactref element="HDMI" pad="17"/>
<contactref element="HDMI" pad="P$1"/>
<contactref element="HDMI" pad="P$2"/>
<contactref element="HDMI" pad="P$3"/>
<contactref element="HDMI" pad="P$4"/>
</signal>
<signal name="3V3">
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JTAG" pad="4"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="XTL" pad="P$1"/>
<contactref element="XTL" pad="P$4"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="VIDEODACSA" pad="30"/>
<contactref element="VIDEODACSA" pad="29"/>
<contactref element="VIDEODACSA" pad="13"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="GPIO_A" pad="29"/>
<contactref element="GPIO_B" pad="29"/>
<contactref element="GPIO_C" pad="29"/>
<contactref element="GPIO_A" pad="29"/>
<contactref element="GPIO_B" pad="29"/>
<contactref element="GPIO_C" pad="29"/>
<contactref element="SDRAM" pad="1"/>
<contactref element="SDRAM" pad="14"/>
<contactref element="SDRAM" pad="27"/>
<contactref element="SDRAM" pad="3"/>
<contactref element="SDRAM" pad="9"/>
<contactref element="SDRAM" pad="43"/>
<contactref element="SDRAM" pad="49"/>
<contactref element="L1" pad="2"/>
<contactref element="3.3V" pad="4"/>
<contactref element="C24" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="VIDEODACSA" pad="38"/>
<contactref element="U$1" pad="L6"/>
<contactref element="U$1" pad="J6"/>
<contactref element="U$1" pad="F3"/>
<contactref element="U$1" pad="E8"/>
<contactref element="U$1" pad="AA21"/>
<contactref element="U$1" pad="F21"/>
<contactref element="U$1" pad="R18"/>
<contactref element="U$1" pad="G7"/>
<contactref element="U$1" pad="P20"/>
<contactref element="U$1" pad="W10"/>
<contactref element="U$1" pad="W15"/>
<contactref element="U$1" pad="T6"/>
<contactref element="U$1" pad="R8"/>
<contactref element="U$1" pad="Y8"/>
<contactref element="U$1" pad="C22"/>
<contactref element="U$1" pad="C7"/>
<contactref element="U$1" pad="M19"/>
<contactref element="U$1" pad="W20"/>
<contactref element="U$1" pad="AA16"/>
<contactref element="U$1" pad="C12"/>
<contactref element="U$1" pad="U14"/>
<contactref element="U$1" pad="F11"/>
<contactref element="U$1" pad="K18"/>
<contactref element="U$1" pad="G14"/>
<contactref element="U$1" pad="R1"/>
<contactref element="U$1" pad="D4"/>
<contactref element="U$1" pad="E18"/>
<contactref element="U$1" pad="Y13"/>
<contactref element="U$1" pad="A16"/>
<contactref element="U$1" pad="J1"/>
<contactref element="U$1" pad="U19"/>
<contactref element="U$1" pad="A6"/>
<contactref element="U$1" pad="D15"/>
<contactref element="U$1" pad="B19"/>
<contactref element="U$1" pad="H17"/>
<contactref element="U$1" pad="T11"/>
<contactref element="U$1" pad="Y4"/>
<contactref element="U$1" pad="N18"/>
<contactref element="U$1" pad="D16"/>
<contactref element="U$1" pad="E1"/>
<contactref element="U$1" pad="W6"/>
<contactref element="U$1" pad="R19"/>
<contactref element="U$1" pad="P21"/>
<contactref element="U$1" pad="V8"/>
<contactref element="U$1" pad="J2"/>
<contactref element="U$1" pad="F8"/>
<contactref element="U$1" pad="W11"/>
<contactref element="U$1" pad="M17"/>
<contactref element="U$1" pad="D8"/>
<contactref element="U$1" pad="E11"/>
<contactref element="U$1" pad="W14"/>
<contactref element="U$1" pad="R2"/>
<contactref element="U$1" pad="W17"/>
<contactref element="U$1" pad="D14"/>
<contactref element="U$1" pad="C10"/>
<contactref element="U$1" pad="W12"/>
<contactref element="U$1" pad="AB16"/>
<contactref element="U$1" pad="B8"/>
<contactref element="U$1" pad="C14"/>
<contactref element="U$1" pad="Y7"/>
<contactref element="U$1" pad="L20"/>
<contactref element="U$1" pad="W1"/>
<contactref element="U$1" pad="R20"/>
<contactref element="U$1" pad="Y12"/>
<contactref element="C28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="SPI" pad="L$2"/>
<contactref element="SPI" pad="8"/>
<contactref element="3.3/2.5/1.1/GND" pad="1"/>
<contactref element="R38" pad="2"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="1V1">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="L14"/>
<contactref element="U$1" pad="P13"/>
<contactref element="U$1" pad="N4"/>
<contactref element="U$1" pad="K13"/>
<contactref element="U$1" pad="J4"/>
<contactref element="U$1" pad="K11"/>
<contactref element="U$1" pad="K15"/>
<contactref element="U$1" pad="M13"/>
<contactref element="U$1" pad="P3"/>
<contactref element="U$1" pad="N10"/>
<contactref element="U$1" pad="P11"/>
<contactref element="U$1" pad="M15"/>
<contactref element="U$1" pad="K3"/>
<contactref element="U$1" pad="P15"/>
<contactref element="U$1" pad="J14"/>
<contactref element="U$1" pad="N14"/>
<contactref element="U$1" pad="J16"/>
<contactref element="U$1" pad="L12"/>
<contactref element="U$1" pad="J10"/>
<contactref element="U$1" pad="K5"/>
<contactref element="U$1" pad="J12"/>
<contactref element="U$1" pad="L10"/>
<contactref element="U$1" pad="N12"/>
<contactref element="U$1" pad="L16"/>
<contactref element="U$1" pad="M11"/>
<contactref element="U$1" pad="L4"/>
<contactref element="C8" pad="2"/>
<contactref element="C37" pad="1"/>
<contactref element="R36" pad="2"/>
<contactref element="L3" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="3.3/2.5/1.1/GND" pad="3"/>
</signal>
<signal name="2V5">
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="2.5V" pad="4"/>
<contactref element="C25" pad="1"/>
<contactref element="U$1" pad="T3"/>
<contactref element="U$1" pad="U18"/>
<contactref element="U$1" pad="H19"/>
<contactref element="U$1" pad="M3"/>
<contactref element="U$1" pad="F4"/>
<contactref element="U$1" pad="T5"/>
<contactref element="U$1" pad="W18"/>
<contactref element="U$1" pad="D18"/>
<contactref element="U$1" pad="D11"/>
<contactref element="U$1" pad="W13"/>
<contactref element="U$1" pad="E6"/>
<contactref element="U$1" pad="W7"/>
<contactref element="U$1" pad="A3"/>
<contactref element="C4" pad="2"/>
<contactref element="3.3/2.5/1.1/GND" pad="2"/>
</signal>
<signal name="CONF_DONE">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="K6"/>
</signal>
<signal name="CONFIG_N">
<contactref element="U$1" pad="A4"/>
<contactref element="R3" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="RESET" pad="1"/>
</signal>
<signal name="TCK">
<contactref element="JTAG" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="V5"/>
</signal>
<signal name="TDO">
<contactref element="JTAG" pad="3"/>
<contactref element="U$1" pad="M5"/>
</signal>
<signal name="TMS">
<contactref element="R6" pad="1"/>
<contactref element="JTAG" pad="5"/>
<contactref element="U$1" pad="P5"/>
</signal>
<signal name="TDI">
<contactref element="R5" pad="1"/>
<contactref element="JTAG" pad="9"/>
<contactref element="U$1" pad="W5"/>
</signal>
<signal name="STATUS_N">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="H5"/>
</signal>
<signal name="RREF_TL">
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="V3"/>
<contactref element="SPI" pad="6"/>
<contactref element="SPI" pad="L$16"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="R4"/>
<contactref element="SPI" pad="L$7"/>
<contactref element="SPI" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="AB3"/>
<contactref element="SPI" pad="L$8"/>
<contactref element="SPI" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="AB4"/>
<contactref element="SPI" pad="L$15"/>
<contactref element="SPI" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="2"/>
<contactref element="SPI" pad="3"/>
<contactref element="SPI" pad="L$9"/>
</signal>
<signal name="N$11">
<contactref element="R10" pad="2"/>
<contactref element="SPI" pad="7"/>
<contactref element="SPI" pad="L$1"/>
</signal>
<signal name="N$12">
<contactref element="XTL" pad="P$3"/>
<contactref element="U$1" pad="H16"/>
</signal>
<signal name="N$13">
<contactref element="VIDEODACSA" pad="34"/>
<contactref element="VGA" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="S-VIDEO" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="VIDEODACSA" pad="32"/>
<contactref element="VGA" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="S-VIDEO" pad="4"/>
</signal>
<signal name="VGA_R0">
<contactref element="VIDEODACSA" pad="41"/>
<contactref element="U$1" pad="A5"/>
<contactref element="RN28" pad="1"/>
</signal>
<signal name="VGA_R1">
<contactref element="VIDEODACSA" pad="42"/>
<contactref element="U$1" pad="B5"/>
<contactref element="RN28" pad="2"/>
</signal>
<signal name="VGA_R2">
<contactref element="VIDEODACSA" pad="43"/>
<contactref element="U$1" pad="B6"/>
</signal>
<signal name="VGA_R3">
<contactref element="VIDEODACSA" pad="44"/>
<contactref element="U$1" pad="D6"/>
<contactref element="RN28" pad="4"/>
</signal>
<signal name="VGA_R4">
<contactref element="VIDEODACSA" pad="45"/>
<contactref element="U$1" pad="C6"/>
<contactref element="RN28" pad="3"/>
</signal>
<signal name="VGA_R5">
<contactref element="VIDEODACSA" pad="46"/>
<contactref element="U$1" pad="A7"/>
</signal>
<signal name="VGA_R6">
<contactref element="VIDEODACSA" pad="47"/>
<contactref element="U$1" pad="B7"/>
</signal>
<signal name="VGA_R7">
<contactref element="VIDEODACSA" pad="48"/>
<contactref element="U$1" pad="E7"/>
</signal>
<signal name="VGA_G0">
<contactref element="VIDEODACSA" pad="3"/>
<contactref element="U$1" pad="D7"/>
</signal>
<signal name="VGA_G1">
<contactref element="VIDEODACSA" pad="4"/>
<contactref element="U$1" pad="F7"/>
</signal>
<signal name="VGA_G2">
<contactref element="VIDEODACSA" pad="5"/>
<contactref element="U$1" pad="A8"/>
</signal>
<signal name="VGA_G3">
<contactref element="VIDEODACSA" pad="6"/>
<contactref element="U$1" pad="G8"/>
</signal>
<signal name="VGA_G4">
<contactref element="VIDEODACSA" pad="7"/>
<contactref element="U$1" pad="C8"/>
</signal>
<signal name="VGA_G5">
<contactref element="VIDEODACSA" pad="8"/>
<contactref element="U$1" pad="H8"/>
</signal>
<signal name="VGA_G6">
<contactref element="VIDEODACSA" pad="9"/>
<contactref element="U$1" pad="A9"/>
</signal>
<signal name="VGA_G7">
<contactref element="VIDEODACSA" pad="10"/>
<contactref element="U$1" pad="D9"/>
</signal>
<signal name="VGA_B0">
<contactref element="VIDEODACSA" pad="16"/>
<contactref element="U$1" pad="E9"/>
</signal>
<signal name="VGA_B1">
<contactref element="VIDEODACSA" pad="17"/>
<contactref element="U$1" pad="F9"/>
<contactref element="RN29" pad="2"/>
</signal>
<signal name="VGA_B2">
<contactref element="VIDEODACSA" pad="18"/>
<contactref element="U$1" pad="A10"/>
</signal>
<signal name="VGA_B3">
<contactref element="VIDEODACSA" pad="19"/>
<contactref element="U$1" pad="B10"/>
</signal>
<signal name="VGA_B4">
<contactref element="VIDEODACSA" pad="20"/>
<contactref element="U$1" pad="E10"/>
<contactref element="RN29" pad="1"/>
</signal>
<signal name="VGA_B5">
<contactref element="VIDEODACSA" pad="21"/>
<contactref element="U$1" pad="F10"/>
<contactref element="RN29" pad="4"/>
</signal>
<signal name="VGA_B6">
<contactref element="VIDEODACSA" pad="22"/>
<contactref element="U$1" pad="G10"/>
<contactref element="RN29" pad="3"/>
</signal>
<signal name="VGA_B7">
<contactref element="VIDEODACSA" pad="23"/>
<contactref element="U$1" pad="B11"/>
</signal>
<signal name="VGA_BLANK_N">
<contactref element="VIDEODACSA" pad="11"/>
<contactref element="U$1" pad="C9"/>
</signal>
<signal name="VGA_CLK">
<contactref element="VIDEODACSA" pad="24"/>
<contactref element="U$1" pad="G11"/>
</signal>
<signal name="N$16">
<contactref element="VIDEODACSA" pad="36"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="VIDEODACSA" pad="37"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="VIDEODACSA" pad="35"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="5V0">
<contactref element="USB.A" pad="VBUS"/>
<contactref element="USB.B" pad="VBUS"/>
<contactref element="PS/2" pad="4"/>
<contactref element="GPIO_A" pad="11"/>
<contactref element="GPIO_B" pad="11"/>
<contactref element="GPIO_C" pad="11"/>
<contactref element="GPIO_A" pad="11"/>
<contactref element="GPIO_B" pad="11"/>
<contactref element="GPIO_C" pad="11"/>
<contactref element="2.5V" pad="1"/>
<contactref element="1.1V" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="3.3V" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="ADC" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="POWER_SW" pad="P$3"/>
<contactref element="HDMI" pad="18"/>
</signal>
<signal name="N$20">
<contactref element="USB.A" pad="D+"/>
<contactref element="R19" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="R16" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="USB.A" pad="D-"/>
</signal>
<signal name="N$25">
<contactref element="R17" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="USB.B" pad="D+"/>
</signal>
<signal name="N$26">
<contactref element="USB.B" pad="D-"/>
<contactref element="R22" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="USB1DP">
<contactref element="R15" pad="1"/>
<contactref element="U$1" pad="V10"/>
</signal>
<signal name="USB1DM">
<contactref element="R16" pad="1"/>
<contactref element="U$1" pad="AA10"/>
</signal>
<signal name="USB2DP">
<contactref element="R17" pad="1"/>
<contactref element="U$1" pad="AB10"/>
</signal>
<signal name="USB2DM">
<contactref element="R18" pad="1"/>
<contactref element="U$1" pad="R11"/>
</signal>
<signal name="SD_DETECT">
<contactref element="U$2" pad="CD"/>
<contactref element="U$1" pad="T13"/>
</signal>
<signal name="SD_WRITEPROTECT">
<contactref element="U$2" pad="WP"/>
<contactref element="U$1" pad="U13"/>
</signal>
<signal name="SD_CS">
<contactref element="U$2" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="U$1" pad="R12"/>
</signal>
<signal name="SD_MOSI">
<contactref element="U$2" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="U$1" pad="T12"/>
</signal>
<signal name="SD_MISO">
<contactref element="U$2" pad="7"/>
<contactref element="R23" pad="1"/>
<contactref element="U$1" pad="AA12"/>
</signal>
<signal name="SD_SCK">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="U12"/>
</signal>
<signal name="PS2DAT">
<contactref element="ZD1" pad="3"/>
<contactref element="R26" pad="1"/>
<contactref element="U$1" pad="Y11"/>
</signal>
<signal name="PS2CLK">
<contactref element="ZD2" pad="3"/>
<contactref element="R27" pad="1"/>
<contactref element="U$1" pad="U11"/>
</signal>
<signal name="N$19">
<contactref element="PS/2" pad="5"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R26" pad="2"/>
<contactref element="PS/2" pad="1"/>
</signal>
<signal name="AUDIO_RIGHT">
<contactref element="R29" pad="2"/>
<contactref element="U$1" pad="A12"/>
</signal>
<signal name="AUDIO_LEFT">
<contactref element="R28" pad="2"/>
<contactref element="U$1" pad="J11"/>
</signal>
<signal name="GPIOC0">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$1" pad="B12"/>
<contactref element="RN9" pad="1"/>
</signal>
<signal name="GPIOC1">
<contactref element="U$3" pad="P$2"/>
<contactref element="U$1" pad="D12"/>
<contactref element="RN9" pad="2"/>
</signal>
<signal name="GPIOC2">
<contactref element="U$3" pad="P$3"/>
<contactref element="U$1" pad="E12"/>
<contactref element="RN9" pad="3"/>
</signal>
<signal name="GPIOC3">
<contactref element="U$3" pad="P$4"/>
<contactref element="U$1" pad="F12"/>
<contactref element="RN9" pad="4"/>
</signal>
<signal name="GPIOC4">
<contactref element="U$3" pad="P$5"/>
<contactref element="U$1" pad="A13"/>
<contactref element="RN10" pad="1"/>
</signal>
<signal name="GPIOC5">
<contactref element="U$3" pad="P$6"/>
<contactref element="U$1" pad="B13"/>
<contactref element="RN10" pad="2"/>
</signal>
<signal name="GPIOC6">
<contactref element="U$3" pad="P$7"/>
<contactref element="U$1" pad="D13"/>
<contactref element="RN10" pad="3"/>
</signal>
<signal name="GPIOC7">
<contactref element="U$3" pad="P$8"/>
<contactref element="U$1" pad="C13"/>
<contactref element="RN10" pad="4"/>
</signal>
<signal name="GPIOC8">
<contactref element="U$3" pad="P$9"/>
<contactref element="U$1" pad="F13"/>
<contactref element="RN11" pad="1"/>
</signal>
<signal name="GPIOC9">
<contactref element="U$3" pad="P$10"/>
<contactref element="U$1" pad="G13"/>
<contactref element="RN11" pad="2"/>
</signal>
<signal name="GPIOC10">
<contactref element="U$3" pad="P$11"/>
<contactref element="U$1" pad="A14"/>
<contactref element="RN11" pad="3"/>
</signal>
<signal name="GPIOC11">
<contactref element="U$3" pad="P$12"/>
<contactref element="U$1" pad="E14"/>
<contactref element="RN11" pad="4"/>
</signal>
<signal name="GPIOC12">
<contactref element="U$3" pad="P$13"/>
<contactref element="U$1" pad="F14"/>
<contactref element="RN12" pad="1"/>
</signal>
<signal name="GPIOC13">
<contactref element="U$3" pad="P$14"/>
<contactref element="U$1" pad="H14"/>
<contactref element="RN12" pad="2"/>
</signal>
<signal name="GPIOC14">
<contactref element="U$3" pad="P$15"/>
<contactref element="U$1" pad="A15"/>
<contactref element="RN12" pad="3"/>
</signal>
<signal name="GPIOC15">
<contactref element="U$3" pad="P$16"/>
<contactref element="U$1" pad="B15"/>
<contactref element="RN12" pad="4"/>
</signal>
<signal name="GPIOC16">
<contactref element="U$3" pad="P$17"/>
<contactref element="U$1" pad="E15"/>
<contactref element="RN16" pad="1"/>
</signal>
<signal name="GPIOC17">
<contactref element="U$3" pad="P$18"/>
<contactref element="U$1" pad="C15"/>
<contactref element="RN16" pad="2"/>
</signal>
<signal name="GPIOC18">
<contactref element="U$3" pad="P$19"/>
<contactref element="U$1" pad="Y16"/>
<contactref element="RN16" pad="3"/>
</signal>
<signal name="GPIOC19">
<contactref element="U$3" pad="P$20"/>
<contactref element="U$1" pad="V16"/>
<contactref element="RN16" pad="4"/>
</signal>
<signal name="GPIOC20">
<contactref element="U$3" pad="P$21"/>
<contactref element="U$1" pad="W16"/>
<contactref element="RN17" pad="1"/>
</signal>
<signal name="GPIOC21">
<contactref element="U$3" pad="P$22"/>
<contactref element="U$1" pad="U16"/>
<contactref element="RN17" pad="2"/>
</signal>
<signal name="GPIOC22">
<contactref element="U$3" pad="P$23"/>
<contactref element="U$1" pad="AB15"/>
<contactref element="RN17" pad="3"/>
</signal>
<signal name="GPIOC23">
<contactref element="U$3" pad="P$24"/>
<contactref element="U$1" pad="AA15"/>
<contactref element="RN17" pad="4"/>
</signal>
<signal name="GPIOC24">
<contactref element="U$3" pad="P$25"/>
<contactref element="U$1" pad="V15"/>
<contactref element="RN18" pad="1"/>
</signal>
<signal name="GPIOC25">
<contactref element="U$3" pad="P$26"/>
<contactref element="U$1" pad="Y15"/>
<contactref element="RN18" pad="2"/>
</signal>
<signal name="GPIOC26">
<contactref element="U$3" pad="P$27"/>
<contactref element="U$1" pad="U15"/>
<contactref element="RN18" pad="3"/>
</signal>
<signal name="GPIOC27">
<contactref element="U$3" pad="P$28"/>
<contactref element="U$1" pad="T15"/>
<contactref element="RN18" pad="4"/>
</signal>
<signal name="GPIOC28">
<contactref element="U$1" pad="AA14"/>
<contactref element="U$3" pad="P$29"/>
<contactref element="RN19" pad="1"/>
</signal>
<signal name="GPIOC29">
<contactref element="U$1" pad="V14"/>
<contactref element="U$3" pad="P$30"/>
<contactref element="RN19" pad="2"/>
</signal>
<signal name="GPIOC30">
<contactref element="U$3" pad="P$31"/>
<contactref element="U$1" pad="Y14"/>
<contactref element="RN19" pad="3"/>
</signal>
<signal name="GPIOC31">
<contactref element="U$3" pad="P$32"/>
<contactref element="U$1" pad="T14"/>
<contactref element="RN19" pad="4"/>
</signal>
<signal name="GPIOC32">
<contactref element="U$3" pad="P$33"/>
<contactref element="U$1" pad="R14"/>
<contactref element="RN15" pad="1"/>
</signal>
<signal name="GPIOC33">
<contactref element="U$1" pad="AB13"/>
<contactref element="U$3" pad="P$34"/>
<contactref element="RN15" pad="2"/>
</signal>
<signal name="GPIOC34">
<contactref element="U$3" pad="P$35"/>
<contactref element="U$1" pad="AA13"/>
<contactref element="RN15" pad="3"/>
</signal>
<signal name="GPIOC35">
<contactref element="U$3" pad="P$36"/>
<contactref element="U$1" pad="V13"/>
<contactref element="RN15" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="GPIO_A" pad="1"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="GPIOA0">
<contactref element="U$1" pad="F15"/>
<contactref element="RN1" pad="1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="GPIO_A" pad="2"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="N$29">
<contactref element="GPIO_A" pad="3"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="GPIO_A" pad="4"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$31">
<contactref element="GPIO_A" pad="5"/>
<contactref element="RN2" pad="8"/>
</signal>
<signal name="N$32">
<contactref element="GPIO_A" pad="6"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="GPIO_A" pad="7"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="GPIO_A" pad="8"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="N$35">
<contactref element="GPIO_A" pad="9"/>
<contactref element="RN3" pad="8"/>
</signal>
<signal name="N$36">
<contactref element="GPIO_A" pad="10"/>
<contactref element="RN3" pad="7"/>
</signal>
<signal name="N$37">
<contactref element="GPIO_A" pad="13"/>
<contactref element="RN3" pad="6"/>
</signal>
<signal name="N$38">
<contactref element="GPIO_A" pad="14"/>
<contactref element="RN3" pad="5"/>
</signal>
<signal name="N$41">
<contactref element="GPIO_A" pad="16"/>
<contactref element="RN4" pad="7"/>
</signal>
<signal name="N$40">
<contactref element="GPIO_A" pad="17"/>
<contactref element="RN4" pad="6"/>
</signal>
<signal name="N$42">
<contactref element="GPIO_A" pad="18"/>
<contactref element="RN4" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="GPIO_A" pad="19"/>
<contactref element="RN13" pad="8"/>
</signal>
<signal name="N$44">
<contactref element="GPIO_A" pad="20"/>
<contactref element="RN13" pad="7"/>
</signal>
<signal name="N$45">
<contactref element="GPIO_A" pad="21"/>
<contactref element="RN13" pad="6"/>
</signal>
<signal name="N$46">
<contactref element="GPIO_A" pad="22"/>
<contactref element="RN13" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="GPIO_A" pad="23"/>
<contactref element="RN24" pad="8"/>
</signal>
<signal name="N$48">
<contactref element="GPIO_A" pad="25"/>
<contactref element="RN24" pad="6"/>
</signal>
<signal name="N$49">
<contactref element="GPIO_A" pad="24"/>
<contactref element="RN24" pad="7"/>
</signal>
<signal name="N$50">
<contactref element="GPIO_A" pad="26"/>
<contactref element="RN24" pad="5"/>
</signal>
<signal name="N$51">
<contactref element="GPIO_A" pad="27"/>
<contactref element="RN25" pad="8"/>
</signal>
<signal name="N$52">
<contactref element="GPIO_A" pad="28"/>
<contactref element="RN25" pad="7"/>
</signal>
<signal name="N$53">
<contactref element="GPIO_A" pad="31"/>
<contactref element="RN25" pad="6"/>
</signal>
<signal name="N$54">
<contactref element="GPIO_A" pad="32"/>
<contactref element="RN25" pad="5"/>
</signal>
<signal name="N$55">
<contactref element="GPIO_A" pad="33"/>
<contactref element="RN26" pad="8"/>
</signal>
<signal name="N$56">
<contactref element="GPIO_A" pad="34"/>
<contactref element="RN26" pad="7"/>
</signal>
<signal name="N$57">
<contactref element="GPIO_A" pad="35"/>
<contactref element="RN26" pad="6"/>
</signal>
<signal name="N$58">
<contactref element="GPIO_A" pad="36"/>
<contactref element="RN26" pad="5"/>
</signal>
<signal name="N$59">
<contactref element="GPIO_A" pad="37"/>
<contactref element="RN27" pad="8"/>
</signal>
<signal name="N$60">
<contactref element="GPIO_A" pad="38"/>
<contactref element="RN27" pad="7"/>
</signal>
<signal name="N$61">
<contactref element="GPIO_A" pad="39"/>
<contactref element="RN27" pad="6"/>
</signal>
<signal name="N$62">
<contactref element="GPIO_A" pad="40"/>
<contactref element="RN27" pad="5"/>
</signal>
<signal name="GPIOA1">
<contactref element="U$1" pad="B16"/>
<contactref element="RN1" pad="2"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="GPIOA2">
<contactref element="U$1" pad="C16"/>
<contactref element="RN1" pad="3"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="GPIOA3">
<contactref element="U$1" pad="G17"/>
<contactref element="RN1" pad="4"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="GPIOA4">
<contactref element="U$1" pad="G16"/>
<contactref element="RN2" pad="1"/>
<contactref element="U$5" pad="P$5"/>
</signal>
<signal name="GPIOA5">
<contactref element="U$1" pad="J18"/>
<contactref element="RN2" pad="2"/>
<contactref element="U$5" pad="P$6"/>
</signal>
<signal name="GPIOA6">
<contactref element="U$1" pad="J17"/>
<contactref element="RN2" pad="3"/>
<contactref element="U$5" pad="P$7"/>
</signal>
<signal name="GPIOA7">
<contactref element="U$1" pad="K21"/>
<contactref element="RN2" pad="4"/>
<contactref element="U$5" pad="P$8"/>
</signal>
<signal name="GPIOA8">
<contactref element="U$1" pad="K20"/>
<contactref element="RN3" pad="1"/>
<contactref element="U$5" pad="P$9"/>
</signal>
<signal name="GPIOA9">
<contactref element="U$1" pad="K16"/>
<contactref element="RN3" pad="2"/>
<contactref element="U$5" pad="P$10"/>
</signal>
<signal name="GPIOA10">
<contactref element="U$1" pad="L19"/>
<contactref element="RN3" pad="3"/>
<contactref element="U$5" pad="P$11"/>
</signal>
<signal name="GPIOA11">
<contactref element="U$1" pad="L17"/>
<contactref element="RN3" pad="4"/>
<contactref element="U$5" pad="P$12"/>
</signal>
<signal name="GPIOA12">
<contactref element="U$1" pad="M21"/>
<contactref element="RN4" pad="1"/>
<contactref element="U$5" pad="P$13"/>
</signal>
<signal name="GPIOA13">
<contactref element="U$1" pad="M20"/>
<contactref element="RN4" pad="2"/>
<contactref element="U$5" pad="P$14"/>
</signal>
<signal name="GPIOA14">
<contactref element="U$1" pad="N21"/>
<contactref element="RN4" pad="3"/>
<contactref element="U$5" pad="P$15"/>
</signal>
<signal name="GPIOA15">
<contactref element="U$1" pad="N20"/>
<contactref element="RN4" pad="4"/>
<contactref element="U$5" pad="P$16"/>
</signal>
<signal name="GPIOA16">
<contactref element="U$1" pad="P22"/>
<contactref element="RN13" pad="1"/>
<contactref element="U$5" pad="P$17"/>
</signal>
<signal name="GPIOA17">
<contactref element="U$1" pad="P19"/>
<contactref element="RN13" pad="2"/>
<contactref element="U$5" pad="P$18"/>
</signal>
<signal name="GPIOA18">
<contactref element="U$1" pad="P16"/>
<contactref element="RN13" pad="3"/>
<contactref element="U$5" pad="P$19"/>
</signal>
<signal name="GPIOA19">
<contactref element="U$1" pad="R21"/>
<contactref element="RN13" pad="4"/>
<contactref element="U$5" pad="P$20"/>
</signal>
<signal name="GPIOA20">
<contactref element="U$1" pad="R16"/>
<contactref element="RN24" pad="1"/>
<contactref element="U$5" pad="P$21"/>
</signal>
<signal name="GPIOA21">
<contactref element="U$1" pad="T19"/>
<contactref element="RN24" pad="2"/>
<contactref element="U$5" pad="P$22"/>
</signal>
<signal name="GPIOA22">
<contactref element="U$1" pad="T18"/>
<contactref element="RN24" pad="3"/>
<contactref element="U$5" pad="P$23"/>
</signal>
<signal name="GPIOA23">
<contactref element="U$1" pad="U22"/>
<contactref element="RN24" pad="4"/>
<contactref element="U$5" pad="P$24"/>
</signal>
<signal name="GPIOA24">
<contactref element="U$1" pad="U20"/>
<contactref element="RN25" pad="1"/>
<contactref element="U$5" pad="P$25"/>
</signal>
<signal name="GPIOA25">
<contactref element="U$1" pad="V19"/>
<contactref element="RN25" pad="2"/>
<contactref element="U$5" pad="P$26"/>
</signal>
<signal name="GPIOA26">
<contactref element="U$1" pad="W22"/>
<contactref element="RN25" pad="3"/>
<contactref element="U$5" pad="P$27"/>
</signal>
<signal name="GPIOA27">
<contactref element="U$1" pad="Y22"/>
<contactref element="RN25" pad="4"/>
<contactref element="U$5" pad="P$28"/>
</signal>
<signal name="GPIOA28">
<contactref element="U$1" pad="AA22"/>
<contactref element="RN26" pad="1"/>
<contactref element="U$5" pad="P$29"/>
</signal>
<signal name="GPIOA29">
<contactref element="U$1" pad="AB21"/>
<contactref element="RN26" pad="2"/>
<contactref element="U$5" pad="P$30"/>
</signal>
<signal name="GPIOA30">
<contactref element="U$1" pad="AA20"/>
<contactref element="RN26" pad="3"/>
<contactref element="U$5" pad="P$31"/>
</signal>
<signal name="GPIOA31">
<contactref element="U$1" pad="AA19"/>
<contactref element="RN26" pad="4"/>
<contactref element="U$5" pad="P$32"/>
</signal>
<signal name="GPIOA32">
<contactref element="U$1" pad="Y19"/>
<contactref element="RN27" pad="1"/>
<contactref element="U$5" pad="P$33"/>
</signal>
<signal name="GPIOA33">
<contactref element="U$1" pad="AA18"/>
<contactref element="RN27" pad="2"/>
<contactref element="U$5" pad="P$34"/>
</signal>
<signal name="GPIOA34">
<contactref element="U$1" pad="AB17"/>
<contactref element="RN27" pad="3"/>
<contactref element="U$5" pad="P$35"/>
</signal>
<signal name="GPIOA35">
<contactref element="U$1" pad="U17"/>
<contactref element="RN27" pad="4"/>
<contactref element="U$5" pad="P$36"/>
</signal>
<signal name="N$63">
<contactref element="GPIO_B" pad="1"/>
<contactref element="RN5" pad="8"/>
</signal>
<signal name="N$64">
<contactref element="GPIO_B" pad="2"/>
<contactref element="RN5" pad="7"/>
</signal>
<signal name="N$65">
<contactref element="GPIO_B" pad="3"/>
<contactref element="RN5" pad="6"/>
</signal>
<signal name="N$66">
<contactref element="GPIO_B" pad="4"/>
<contactref element="RN5" pad="5"/>
</signal>
<signal name="N$67">
<contactref element="GPIO_B" pad="5"/>
<contactref element="RN6" pad="8"/>
</signal>
<signal name="N$68">
<contactref element="GPIO_B" pad="6"/>
<contactref element="RN6" pad="7"/>
</signal>
<signal name="N$69">
<contactref element="GPIO_B" pad="7"/>
<contactref element="RN6" pad="6"/>
</signal>
<signal name="N$70">
<contactref element="GPIO_B" pad="8"/>
<contactref element="RN6" pad="5"/>
</signal>
<signal name="N$71">
<contactref element="GPIO_B" pad="9"/>
<contactref element="RN7" pad="8"/>
</signal>
<signal name="N$72">
<contactref element="GPIO_B" pad="10"/>
<contactref element="RN7" pad="7"/>
</signal>
<signal name="N$73">
<contactref element="GPIO_B" pad="13"/>
<contactref element="RN7" pad="6"/>
</signal>
<signal name="N$74">
<contactref element="GPIO_B" pad="14"/>
<contactref element="RN7" pad="5"/>
</signal>
<signal name="N$75">
<contactref element="GPIO_B" pad="15"/>
<contactref element="RN8" pad="8"/>
</signal>
<signal name="N$76">
<contactref element="GPIO_B" pad="16"/>
<contactref element="RN8" pad="7"/>
</signal>
<signal name="N$77">
<contactref element="GPIO_B" pad="17"/>
<contactref element="RN8" pad="6"/>
</signal>
<signal name="N$78">
<contactref element="GPIO_B" pad="18"/>
<contactref element="RN8" pad="5"/>
</signal>
<signal name="N$79">
<contactref element="GPIO_B" pad="19"/>
<contactref element="RN14" pad="8"/>
</signal>
<signal name="N$80">
<contactref element="GPIO_B" pad="20"/>
<contactref element="RN14" pad="7"/>
</signal>
<signal name="N$81">
<contactref element="GPIO_B" pad="21"/>
<contactref element="RN14" pad="6"/>
</signal>
<signal name="N$82">
<contactref element="GPIO_B" pad="22"/>
<contactref element="RN14" pad="5"/>
</signal>
<signal name="N$83">
<contactref element="GPIO_B" pad="23"/>
<contactref element="RN20" pad="8"/>
</signal>
<signal name="N$84">
<contactref element="GPIO_B" pad="24"/>
<contactref element="RN20" pad="7"/>
</signal>
<signal name="N$85">
<contactref element="GPIO_B" pad="25"/>
<contactref element="RN20" pad="6"/>
</signal>
<signal name="N$86">
<contactref element="GPIO_B" pad="26"/>
<contactref element="RN20" pad="5"/>
</signal>
<signal name="N$87">
<contactref element="GPIO_B" pad="27"/>
<contactref element="RN21" pad="8"/>
</signal>
<signal name="N$88">
<contactref element="GPIO_B" pad="28"/>
<contactref element="RN21" pad="7"/>
</signal>
<signal name="N$89">
<contactref element="GPIO_B" pad="31"/>
<contactref element="RN21" pad="6"/>
</signal>
<signal name="N$90">
<contactref element="GPIO_B" pad="32"/>
<contactref element="RN21" pad="5"/>
</signal>
<signal name="N$91">
<contactref element="GPIO_B" pad="33"/>
<contactref element="RN22" pad="8"/>
</signal>
<signal name="N$92">
<contactref element="GPIO_B" pad="34"/>
<contactref element="RN22" pad="7"/>
</signal>
<signal name="N$93">
<contactref element="GPIO_B" pad="35"/>
<contactref element="RN22" pad="6"/>
</signal>
<signal name="N$94">
<contactref element="GPIO_B" pad="36"/>
<contactref element="RN22" pad="5"/>
</signal>
<signal name="N$95">
<contactref element="GPIO_B" pad="37"/>
<contactref element="RN23" pad="8"/>
</signal>
<signal name="N$96">
<contactref element="GPIO_B" pad="38"/>
<contactref element="RN23" pad="7"/>
</signal>
<signal name="N$97">
<contactref element="GPIO_B" pad="39"/>
<contactref element="RN23" pad="6"/>
</signal>
<signal name="N$98">
<contactref element="GPIO_B" pad="40"/>
<contactref element="RN23" pad="5"/>
</signal>
<signal name="GPIOB0">
<contactref element="U$1" pad="G15"/>
<contactref element="RN5" pad="1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="GPIOB1">
<contactref element="U$1" pad="E16"/>
<contactref element="RN5" pad="2"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="GPIOB2">
<contactref element="U$1" pad="D17"/>
<contactref element="RN5" pad="3"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="GPIOB3">
<contactref element="U$1" pad="G18"/>
<contactref element="RN5" pad="4"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="GPIOB4">
<contactref element="U$1" pad="H18"/>
<contactref element="RN6" pad="1"/>
<contactref element="U$4" pad="P$5"/>
</signal>
<signal name="GPIOB5">
<contactref element="U$1" pad="J19"/>
<contactref element="RN6" pad="2"/>
<contactref element="U$4" pad="P$6"/>
</signal>
<signal name="GPIOB6">
<contactref element="U$1" pad="K22"/>
<contactref element="RN6" pad="3"/>
<contactref element="U$4" pad="P$7"/>
</signal>
<signal name="GPIOB7">
<contactref element="U$1" pad="K19"/>
<contactref element="RN6" pad="4"/>
<contactref element="U$4" pad="P$8"/>
</signal>
<signal name="GPIOB8">
<contactref element="U$1" pad="K17"/>
<contactref element="RN7" pad="1"/>
<contactref element="U$4" pad="P$9"/>
</signal>
<signal name="GPIOB9">
<contactref element="U$1" pad="L22"/>
<contactref element="RN7" pad="2"/>
<contactref element="U$4" pad="P$10"/>
</signal>
<signal name="GPIOB10">
<contactref element="U$1" pad="L18"/>
<contactref element="RN7" pad="3"/>
<contactref element="U$4" pad="P$11"/>
</signal>
<signal name="GPIOB11">
<contactref element="U$1" pad="M22"/>
<contactref element="RN7" pad="4"/>
<contactref element="U$4" pad="P$12"/>
</signal>
<signal name="GPIOB12">
<contactref element="U$1" pad="M18"/>
<contactref element="RN8" pad="1"/>
<contactref element="U$4" pad="P$13"/>
</signal>
<signal name="GPIOB13">
<contactref element="U$1" pad="M16"/>
<contactref element="RN8" pad="2"/>
<contactref element="U$4" pad="P$14"/>
</signal>
<signal name="GPIOB14">
<contactref element="U$1" pad="N19"/>
<contactref element="RN8" pad="3"/>
<contactref element="U$4" pad="P$15"/>
</signal>
<signal name="GPIOB15">
<contactref element="U$1" pad="N16"/>
<contactref element="RN8" pad="4"/>
<contactref element="U$4" pad="P$16"/>
</signal>
<signal name="GPIOB16">
<contactref element="U$1" pad="P18"/>
<contactref element="RN14" pad="1"/>
<contactref element="U$4" pad="P$17"/>
</signal>
<signal name="GPIOB17">
<contactref element="U$1" pad="P17"/>
<contactref element="RN14" pad="2"/>
<contactref element="U$4" pad="P$18"/>
</signal>
<signal name="GPIOB18">
<contactref element="U$1" pad="R22"/>
<contactref element="RN14" pad="3"/>
<contactref element="U$4" pad="P$19"/>
</signal>
<signal name="GPIOB19">
<contactref element="U$1" pad="R17"/>
<contactref element="RN14" pad="4"/>
<contactref element="U$4" pad="P$20"/>
</signal>
<signal name="GPIOB20">
<contactref element="U$1" pad="T22"/>
<contactref element="RN20" pad="1"/>
<contactref element="U$4" pad="P$21"/>
</signal>
<signal name="GPIOB21">
<contactref element="U$1" pad="T20"/>
<contactref element="RN20" pad="2"/>
<contactref element="U$4" pad="P$22"/>
</signal>
<signal name="GPIOB22">
<contactref element="U$1" pad="T17"/>
<contactref element="RN20" pad="3"/>
<contactref element="U$4" pad="P$23"/>
</signal>
<signal name="GPIOB23">
<contactref element="U$1" pad="U21"/>
<contactref element="RN20" pad="4"/>
<contactref element="U$4" pad="P$24"/>
</signal>
<signal name="GPIOB24">
<contactref element="U$1" pad="V21"/>
<contactref element="RN21" pad="1"/>
<contactref element="U$4" pad="P$25"/>
</signal>
<signal name="GPIOB25">
<contactref element="U$1" pad="V20"/>
<contactref element="RN21" pad="2"/>
<contactref element="U$4" pad="P$26"/>
</signal>
<signal name="GPIOB26">
<contactref element="U$1" pad="W21"/>
<contactref element="RN21" pad="3"/>
<contactref element="U$4" pad="P$27"/>
</signal>
<signal name="GPIOB27">
<contactref element="U$1" pad="Y21"/>
<contactref element="RN21" pad="4"/>
<contactref element="U$4" pad="P$28"/>
</signal>
<signal name="GPIOB28">
<contactref element="U$1" pad="AB22"/>
<contactref element="RN22" pad="1"/>
<contactref element="U$4" pad="P$29"/>
</signal>
<signal name="GPIOB29">
<contactref element="U$1" pad="AB20"/>
<contactref element="RN22" pad="2"/>
<contactref element="U$4" pad="P$30"/>
</signal>
<signal name="GPIOB30">
<contactref element="U$1" pad="Y20"/>
<contactref element="RN22" pad="3"/>
<contactref element="U$4" pad="P$31"/>
</signal>
<signal name="GPIOB31">
<contactref element="U$1" pad="W19"/>
<contactref element="RN22" pad="4"/>
<contactref element="U$4" pad="P$32"/>
</signal>
<signal name="GPIOB32">
<contactref element="U$1" pad="AB18"/>
<contactref element="RN23" pad="1"/>
<contactref element="U$4" pad="P$33"/>
</signal>
<signal name="GPIOB33">
<contactref element="U$1" pad="V18"/>
<contactref element="RN23" pad="2"/>
<contactref element="U$4" pad="P$34"/>
</signal>
<signal name="GPIOB34">
<contactref element="U$1" pad="AA17"/>
<contactref element="RN23" pad="3"/>
<contactref element="U$4" pad="P$35"/>
</signal>
<signal name="GPIOB35">
<contactref element="U$1" pad="Y17"/>
<contactref element="RN23" pad="4"/>
<contactref element="U$4" pad="P$36"/>
</signal>
<signal name="A0">
<contactref element="SDRAM" pad="23"/>
<contactref element="U$1" pad="R6"/>
</signal>
<signal name="A1">
<contactref element="SDRAM" pad="24"/>
<contactref element="U$1" pad="R5"/>
</signal>
<signal name="A2">
<contactref element="SDRAM" pad="25"/>
<contactref element="U$1" pad="T7"/>
</signal>
<signal name="A3">
<contactref element="SDRAM" pad="26"/>
<contactref element="U$1" pad="U6"/>
</signal>
<signal name="A4">
<contactref element="SDRAM" pad="29"/>
<contactref element="U$1" pad="Y10"/>
</signal>
<signal name="A5">
<contactref element="SDRAM" pad="30"/>
<contactref element="U$1" pad="U10"/>
</signal>
<signal name="A6">
<contactref element="SDRAM" pad="31"/>
<contactref element="U$1" pad="T10"/>
</signal>
<signal name="A7">
<contactref element="SDRAM" pad="32"/>
<contactref element="U$1" pad="AA9"/>
</signal>
<signal name="A8">
<contactref element="SDRAM" pad="33"/>
<contactref element="U$1" pad="W9"/>
</signal>
<signal name="A9">
<contactref element="SDRAM" pad="34"/>
<contactref element="U$1" pad="Y9"/>
</signal>
<signal name="A10">
<contactref element="SDRAM" pad="22"/>
<contactref element="U$1" pad="R7"/>
</signal>
<signal name="A11">
<contactref element="SDRAM" pad="35"/>
<contactref element="U$1" pad="V9"/>
</signal>
<signal name="A12">
<contactref element="SDRAM" pad="36"/>
<contactref element="U$1" pad="T9"/>
</signal>
<signal name="BA0">
<contactref element="SDRAM" pad="20"/>
<contactref element="U$1" pad="P7"/>
</signal>
<signal name="BA1">
<contactref element="SDRAM" pad="21"/>
<contactref element="U$1" pad="P6"/>
</signal>
<signal name="SDRAM_UDQM">
<contactref element="SDRAM" pad="39"/>
<contactref element="U$1" pad="U8"/>
</signal>
<signal name="SDRAM_LDQM">
<contactref element="SDRAM" pad="15"/>
<contactref element="U$1" pad="M6"/>
</signal>
<signal name="SDRAM_CLK">
<contactref element="SDRAM" pad="38"/>
<contactref element="U$1" pad="AA8"/>
</signal>
<signal name="CKE">
<contactref element="SDRAM" pad="37"/>
<contactref element="U$1" pad="AB8"/>
</signal>
<signal name="CS_N">
<contactref element="SDRAM" pad="19"/>
<contactref element="U$1" pad="P8"/>
</signal>
<signal name="RAS_N">
<contactref element="SDRAM" pad="18"/>
<contactref element="U$1" pad="N6"/>
</signal>
<signal name="CAS_N">
<contactref element="SDRAM" pad="17"/>
<contactref element="U$1" pad="N8"/>
</signal>
<signal name="WE_N">
<contactref element="SDRAM" pad="16"/>
<contactref element="U$1" pad="N9"/>
</signal>
<signal name="DQ0">
<contactref element="SDRAM" pad="2"/>
<contactref element="U$1" pad="K7"/>
</signal>
<signal name="DQ1">
<contactref element="SDRAM" pad="4"/>
<contactref element="U$1" pad="K9"/>
</signal>
<signal name="DQ2">
<contactref element="SDRAM" pad="5"/>
<contactref element="U$1" pad="J7"/>
</signal>
<signal name="DQ3">
<contactref element="SDRAM" pad="7"/>
<contactref element="U$1" pad="J8"/>
</signal>
<signal name="DQ4">
<contactref element="SDRAM" pad="8"/>
<contactref element="U$1" pad="L8"/>
</signal>
<signal name="DQ5">
<contactref element="SDRAM" pad="10"/>
<contactref element="U$1" pad="L7"/>
</signal>
<signal name="DQ6">
<contactref element="SDRAM" pad="11"/>
<contactref element="U$1" pad="M8"/>
</signal>
<signal name="DQ7">
<contactref element="SDRAM" pad="13"/>
<contactref element="U$1" pad="M7"/>
</signal>
<signal name="DQ8">
<contactref element="SDRAM" pad="42"/>
<contactref element="U$1" pad="W8"/>
</signal>
<signal name="DQ9">
<contactref element="SDRAM" pad="44"/>
<contactref element="U$1" pad="T8"/>
</signal>
<signal name="DQ10">
<contactref element="SDRAM" pad="45"/>
<contactref element="U$1" pad="AB7"/>
</signal>
<signal name="DQ11">
<contactref element="SDRAM" pad="47"/>
<contactref element="U$1" pad="AA7"/>
</signal>
<signal name="DQ12">
<contactref element="SDRAM" pad="48"/>
<contactref element="U$1" pad="U7"/>
</signal>
<signal name="DQ13">
<contactref element="SDRAM" pad="50"/>
<contactref element="U$1" pad="AB6"/>
</signal>
<signal name="DQ14">
<contactref element="SDRAM" pad="51"/>
<contactref element="U$1" pad="V6"/>
</signal>
<signal name="DQ15">
<contactref element="SDRAM" pad="53"/>
<contactref element="U$1" pad="AB5"/>
</signal>
<signal name="N$135">
<contactref element="1.1V" pad="5"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="N$136">
<contactref element="2.5V" pad="5"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$137">
<contactref element="3.3V" pad="5"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="SD_DAT1">
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="AB12"/>
</signal>
<signal name="SD_DAT2">
<contactref element="U$2" pad="9"/>
<contactref element="U$1" pad="AB11"/>
</signal>
<signal name="N$39">
<contactref element="GPIO_A" pad="15"/>
<contactref element="RN4" pad="8"/>
</signal>
<signal name="VSYNC">
<contactref element="U$1" pad="H11"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="HSYNC">
<contactref element="U$1" pad="C11"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$140">
</signal>
<signal name="N$2">
<contactref element="5V_IN_B" pad="VBUS"/>
<contactref element="PF1" pad="1"/>
<contactref element="5V_IN" pad="P$1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="H6"/>
<contactref element="ADC" pad="4"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="G6"/>
<contactref element="ADC" pad="5"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="5V0FAST">
<contactref element="R30" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="1.1V" pad="3"/>
</signal>
<signal name="5V0SLOW">
<contactref element="R7" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="3.3V" pad="3"/>
<contactref element="2.5V" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="VGA" pad="14"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="VGA" pad="13"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$139">
<contactref element="PF1" pad="2"/>
<contactref element="POWER_SW" pad="P$2"/>
</signal>
<signal name="AUDIO_IN">
<contactref element="ADC" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R29" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R28" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="R34" pad="2"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$138">
<contactref element="C35" pad="1"/>
<contactref element="AUDIO" pad="P$3"/>
</signal>
<signal name="N$141">
<contactref element="C36" pad="1"/>
<contactref element="AUDIO" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="R33" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="N$142">
<contactref element="C34" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="C36" pad="2"/>
</signal>
<signal name="GNDOFF">
</signal>
<signal name="N$145">
<contactref element="R36" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="1.1V" pad="4"/>
</signal>
<signal name="N$143">
<contactref element="C-VIDEO" pad="1"/>
<contactref element="VIDEODACSA" pad="28"/>
<contactref element="VGA" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="GPIO_C" pad="1"/>
<contactref element="RN9" pad="8"/>
</signal>
<signal name="N$99">
<contactref element="GPIO_C" pad="2"/>
<contactref element="RN9" pad="7"/>
</signal>
<signal name="N$100">
<contactref element="RN9" pad="6"/>
<contactref element="GPIO_C" pad="3"/>
</signal>
<signal name="N$101">
<contactref element="GPIO_C" pad="4"/>
<contactref element="RN9" pad="5"/>
</signal>
<signal name="N$102">
<contactref element="RN10" pad="8"/>
<contactref element="GPIO_C" pad="5"/>
</signal>
<signal name="N$103">
<contactref element="GPIO_C" pad="6"/>
<contactref element="RN10" pad="7"/>
</signal>
<signal name="N$104">
<contactref element="GPIO_C" pad="7"/>
<contactref element="RN10" pad="6"/>
</signal>
<signal name="N$105">
<contactref element="RN10" pad="5"/>
<contactref element="GPIO_C" pad="8"/>
</signal>
<signal name="N$106">
<contactref element="GPIO_C" pad="9"/>
<contactref element="RN11" pad="8"/>
</signal>
<signal name="N$107">
<contactref element="RN11" pad="7"/>
<contactref element="GPIO_C" pad="10"/>
</signal>
<signal name="N$108">
<contactref element="GPIO_C" pad="13"/>
<contactref element="RN11" pad="6"/>
</signal>
<signal name="N$109">
<contactref element="RN11" pad="5"/>
<contactref element="GPIO_C" pad="14"/>
</signal>
<signal name="N$110">
<contactref element="GPIO_C" pad="15"/>
<contactref element="RN12" pad="8"/>
</signal>
<signal name="N$111">
<contactref element="RN12" pad="7"/>
<contactref element="GPIO_C" pad="16"/>
</signal>
<signal name="N$112">
<contactref element="GPIO_C" pad="17"/>
<contactref element="RN12" pad="6"/>
</signal>
<signal name="N$113">
<contactref element="RN12" pad="5"/>
<contactref element="GPIO_C" pad="18"/>
</signal>
<signal name="N$114">
<contactref element="RN16" pad="8"/>
<contactref element="GPIO_C" pad="19"/>
</signal>
<signal name="N$115">
<contactref element="GPIO_C" pad="20"/>
<contactref element="RN16" pad="7"/>
</signal>
<signal name="N$116">
<contactref element="RN16" pad="6"/>
<contactref element="GPIO_C" pad="21"/>
</signal>
<signal name="N$117">
<contactref element="GPIO_C" pad="22"/>
<contactref element="RN16" pad="5"/>
</signal>
<signal name="N$118">
<contactref element="RN17" pad="8"/>
<contactref element="GPIO_C" pad="23"/>
</signal>
<signal name="N$119">
<contactref element="GPIO_C" pad="24"/>
<contactref element="RN17" pad="7"/>
</signal>
<signal name="N$120">
<contactref element="RN17" pad="6"/>
<contactref element="GPIO_C" pad="25"/>
</signal>
<signal name="N$121">
<contactref element="GPIO_C" pad="26"/>
<contactref element="RN17" pad="5"/>
</signal>
<signal name="N$122">
<contactref element="RN18" pad="8"/>
<contactref element="GPIO_C" pad="27"/>
</signal>
<signal name="N$123">
<contactref element="GPIO_C" pad="28"/>
<contactref element="RN18" pad="7"/>
</signal>
<signal name="N$124">
<contactref element="RN18" pad="6"/>
<contactref element="GPIO_C" pad="31"/>
</signal>
<signal name="N$125">
<contactref element="GPIO_C" pad="32"/>
<contactref element="RN18" pad="5"/>
</signal>
<signal name="N$126">
<contactref element="RN19" pad="8"/>
<contactref element="GPIO_C" pad="33"/>
</signal>
<signal name="N$127">
<contactref element="GPIO_C" pad="34"/>
<contactref element="RN19" pad="7"/>
</signal>
<signal name="N$128">
<contactref element="RN19" pad="6"/>
<contactref element="GPIO_C" pad="35"/>
</signal>
<signal name="N$129">
<contactref element="GPIO_C" pad="36"/>
<contactref element="RN19" pad="5"/>
</signal>
<signal name="N$130">
<contactref element="GPIO_C" pad="37"/>
<contactref element="RN15" pad="8"/>
</signal>
<signal name="N$131">
<contactref element="RN15" pad="7"/>
<contactref element="GPIO_C" pad="38"/>
</signal>
<signal name="N$132">
<contactref element="GPIO_C" pad="39"/>
<contactref element="RN15" pad="6"/>
</signal>
<signal name="N$133">
<contactref element="RN15" pad="5"/>
<contactref element="GPIO_C" pad="40"/>
</signal>
<signal name="N$134">
<contactref element="RN28" pad="8"/>
<contactref element="HDMI" pad="1"/>
</signal>
<signal name="N$144">
<contactref element="HDMI" pad="3"/>
<contactref element="RN28" pad="7"/>
</signal>
<signal name="N$146">
<contactref element="RN28" pad="6"/>
<contactref element="HDMI" pad="4"/>
</signal>
<signal name="N$147">
<contactref element="HDMI" pad="6"/>
<contactref element="RN28" pad="5"/>
</signal>
<signal name="N$148">
<contactref element="RN29" pad="8"/>
<contactref element="HDMI" pad="7"/>
</signal>
<signal name="N$149">
<contactref element="HDMI" pad="9"/>
<contactref element="RN29" pad="7"/>
</signal>
<signal name="N$150">
<contactref element="RN29" pad="6"/>
<contactref element="HDMI" pad="10"/>
</signal>
<signal name="N$151">
<contactref element="HDMI" pad="12"/>
<contactref element="RN29" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
