<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
<symbols>
<symbol name="SPX3819M5-L">
<pin name="VIN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="ADJ/BYP" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="ADC">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AIN" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SPX3819M5-L" prefix="U">
<description>500mA, LOW-NOISE LDO VOLTAGE REGULATOR</description>
<gates>
<gate name="A" symbol="SPX3819M5-L"/>
</gates>
<devices>
<device name="" package="SOT95P280X145-5N">
<connects>
<connect gate="A" pin="ADJ/BYP" pad="4"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SPX3819M5-L"/>
<attribute name="OC_FARNELL" value="1831948"/>
<attribute name="OC_NEWARK" value="23R9689"/>
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="SUPPLIER" value="EXAR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP3021">
<gates>
<gate name="G$1" symbol="ADC"/>
</gates>
<devices>
<device name="" package="SOT95P280X145-5N">
<connects>
<connect gate="G$1" pin="AIN" pad="3"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
