<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="AUDIO-JACK">
</package>
<package name="AUDIO-JACK-3.5MM-SMD">
</package>
<package name="AUDIO-JACK-KIT">
<description>Kit footprint for 1/8" audio jack.

Reduced openings in tStop, pins spread a tiny bit out to hold part on PCB during assembly</description>
</package>
<package name="AUDIO-JACK-CUI-353X">
</package>
</packages>
<symbols>
<symbol name="AUDIO-JACK2">
<pin name="RING"/>
<pin name="TIP"/>
<pin name="SLEEVE"/>
<pin name="RSH"/>
<pin name="TSH"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AUDIO-JACK2" prefix="J">
<description>Stereo audio jack with bypass switches.&lt;br&gt;
SMT version used on LilyPad MP3 board.&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK2"/>
</gates>
<devices>
<device name="PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08774"/>
</technology>
</technologies>
</device>
<device name="SMD" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10353"/>
</technology>
</technologies>
</device>
<device name="KIT" package="AUDIO-JACK-KIT">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08774"/>
</technology>
</technologies>
</device>
<device name="CUI" package="AUDIO-JACK-CUI-353X">
<connects>
<connect gate="G$1" pin="RING" pad="P$3"/>
<connect gate="G$1" pin="RSH" pad="P$5"/>
<connect gate="G$1" pin="SLEEVE" pad="P$1"/>
<connect gate="G$1" pin="TIP" pad="P$2"/>
<connect gate="G$1" pin="TSH" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
