<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="29.7" y1="53.8" x2="9" y2="53.8" width="0" layer="20"/>
<wire x1="9" y1="53.8" x2="9" y2="1" width="0" layer="20"/>
<wire x1="9" y1="1" x2="29.7" y2="1" width="0" layer="20"/>
<wire x1="29.7" y1="1" x2="29.7" y2="53.8" width="0" layer="20"/>
</plain>
<libraries>
<library name="max10">
<packages>
<package name="U169SMALL">
</package>
<package name="56TVSOP_SMALL">
</package>
<package name="DRY6">
</package>
<package name="TDFN4_1P2X1P6_MCH">
</package>
</packages>
</library>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="R1206-8">
<description>&lt;b&gt;BOURNS&lt;/b&gt; Chip Resistor Array&lt;p&gt;
Source: RS Component / BUORNS</description>
</package>
</packages>
</library>
<library name="resistor-array">
<description>&lt;b&gt;SMD Resistor Arrays&lt;/b&gt;&lt;p&gt;
CTS, Rohm, etc&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="741-8">
<description>CTS 741 Series&lt;p&gt;
8 Terminations, 4 Resistors</description>
</package>
</packages>
</library>
<library name="LQM2HPN1R0MJ0L">
<packages>
<package name="INDC1008X04">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Locking Footprint&lt;/h3&gt;
Holes are offset from center 0.005", to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TSV854IQ4T">
<packages>
<package name="QFN50P300X300X100-16N">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ASE">
<description>&lt;b&gt;3.3Vdc CMOS SMD CRYSTAL CLOCK OSCILLATOR&lt;/b&gt; ASE Series&lt;p&gt;
Source: www.abracon.com</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C8" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0402" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0402" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="max10" package="U169SMALL" value="MAX10">
<attribute name="NAME"/>
</element>
<element name="CN1" library="Discrete" package="R1206-8" value="18nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="rcl" package="R0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="max10" package="56TVSOP_SMALL" value="SN74CB3T16211SM">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="REG1" library="max10" package="DRY6" value="TPS62237DRYR">
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TPS62237DRYR"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="LQM2HPN1R0MJ0L" package="INDC1008X04" value="LQM2HPN1R0MJ0L">
<attribute name="PACKAGE" value="1008 Murata"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/murata-electronics-north-america/LQM2HPN1R0MJ0L/490-6699-1-ND/3845896?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MP" value="LQM2HPN1R0MJ0L"/>
<attribute name="DESCRIPTION" value=" Inductor Power Chip Shielded Multi-Layer 1uH 20% 1MHz Ferrite 1.5A 113mOhm DCR 1008 Embossed T/R "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="DIGI-KEY_PART_NUMBER" value="490-6699-1-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JTAG" library="SparkFun-Connectors" package="2X3_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="TSV854IQ4T" package="QFN50P300X300X100-16N" value="TSV854IQ4T">
<attribute name="PACKAGE" value="QFN-16 STMicroelectronics"/>
<attribute name="MP" value="TSV854IQ4T"/>
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="PRICE" value="None"/>
<attribute name="DESCRIPTION" value=" General Purpose Amplifier 4 Circuit Rail-to-Rail 16-QFN _3x3_ "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0402" value="1k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0402" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REG2" library="max10" package="TDFN4_1P2X1P6_MCH" value="MIC94310-JYMT-TR">
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="SOURCELIBRARY" value="Microchip_2019-08-23_18"/>
<attribute name="VENDOR" value="Microchip"/>
<attribute name="BUILT_BY" value="EMA_Jessica"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIC94310-JYMT-TR"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="C0402" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="resistor-array" package="741-8" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-array" package="741-8" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-array" package="741-8" value="20K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POKEYMAX1" library="ic-package" package="DIL40" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="max10" package="56TVSOP_SMALL" value="SN74CB3T16211SM">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="rcl" package="R0402" value="1k1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="R0402" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="2X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUD" library="pinhead" package="2X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0402" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0402" value="3k3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0402" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="crystal" package="ASE" value="ASE">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U3" pad="A13"/>
<contactref element="U3" pad="A1"/>
<contactref element="U3" pad="B8"/>
<contactref element="U3" pad="E11"/>
<contactref element="U3" pad="F3"/>
<contactref element="U3" pad="C3"/>
<contactref element="U3" pad="H12"/>
<contactref element="U3" pad="D5"/>
<contactref element="U3" pad="G7"/>
<contactref element="U3" pad="N13"/>
<contactref element="U3" pad="M6"/>
<contactref element="U3" pad="J4"/>
<contactref element="U3" pad="N1"/>
<contactref element="U3" pad="L9"/>
<contactref element="CN1" pad="4"/>
<contactref element="CN1" pad="1"/>
<contactref element="CN1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="19"/>
<contactref element="U2" pad="38"/>
<contactref element="U2" pad="49"/>
<contactref element="REG1" pad="4"/>
<contactref element="REG1" pad="1"/>
<contactref element="U2" pad="56"/>
<contactref element="U2" pad="55"/>
<contactref element="JTAG" pad="5"/>
<contactref element="U1" pad="11"/>
<contactref element="REG2" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="REG2" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="RN1" pad="4"/>
<contactref element="RN1" pad="1"/>
<contactref element="RN1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="RN1" pad="2"/>
<contactref element="CN1" pad="2"/>
<contactref element="POKEYMAX1" pad="1"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="38"/>
<contactref element="U4" pad="49"/>
<contactref element="U4" pad="19"/>
<contactref element="U4" pad="56"/>
<contactref element="U4" pad="55"/>
<contactref element="AUD" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="LVLA17">
<contactref element="U2" pad="35"/>
<contactref element="POKEYMAX1" pad="32"/>
</signal>
<signal name="LVLA16">
<contactref element="U2" pad="36"/>
<contactref element="POKEYMAX1" pad="33"/>
</signal>
<signal name="LVLA15">
<contactref element="U2" pad="37"/>
<contactref element="POKEYMAX1" pad="34"/>
</signal>
<signal name="LVLA5">
<contactref element="U2" pad="48"/>
<contactref element="POKEYMAX1" pad="7"/>
</signal>
<signal name="LVLA4">
<contactref element="U2" pad="50"/>
<contactref element="POKEYMAX1" pad="6"/>
</signal>
<signal name="LVLA3">
<contactref element="U2" pad="51"/>
<contactref element="POKEYMAX1" pad="5"/>
</signal>
<signal name="LVLA2">
<contactref element="U2" pad="52"/>
<contactref element="POKEYMAX1" pad="4"/>
</signal>
<signal name="LVLA1">
<contactref element="U2" pad="53"/>
<contactref element="POKEYMAX1" pad="3"/>
</signal>
<signal name="LVLA0">
<contactref element="U2" pad="54"/>
<contactref element="POKEYMAX1" pad="2"/>
</signal>
<signal name="LVLA14">
<contactref element="U2" pad="39"/>
<contactref element="POKEYMAX1" pad="40"/>
</signal>
<signal name="LVLA12">
<contactref element="U2" pad="41"/>
<contactref element="POKEYMAX1" pad="39"/>
</signal>
<signal name="LVLA11">
<contactref element="U2" pad="42"/>
<contactref element="POKEYMAX1" pad="30"/>
</signal>
<signal name="LVLA8">
<contactref element="U2" pad="45"/>
<contactref element="POKEYMAX1" pad="27"/>
</signal>
<signal name="LVLA9">
<contactref element="U2" pad="44"/>
<contactref element="POKEYMAX1" pad="38"/>
</signal>
<signal name="LVLA22">
<contactref element="U2" pad="30"/>
<contactref element="POKEYMAX1" pad="24"/>
</signal>
<signal name="LVLA20">
<contactref element="U2" pad="32"/>
<contactref element="POKEYMAX1" pad="25"/>
</signal>
<signal name="LIN0">
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="B1"/>
</signal>
<signal name="LIN1">
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="A2"/>
</signal>
<signal name="LIN2">
<contactref element="U2" pad="4"/>
<contactref element="U3" pad="B2"/>
</signal>
<signal name="LIN3">
<contactref element="U2" pad="5"/>
<contactref element="U3" pad="A3"/>
</signal>
<signal name="LIN4">
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="B3"/>
</signal>
<signal name="LIN5">
<contactref element="U2" pad="7"/>
<contactref element="U3" pad="A4"/>
</signal>
<signal name="LIN6">
<contactref element="U2" pad="9"/>
<contactref element="U3" pad="B4"/>
</signal>
<signal name="LIN7">
<contactref element="U2" pad="10"/>
<contactref element="U3" pad="A5"/>
</signal>
<signal name="LIN8">
<contactref element="U2" pad="11"/>
<contactref element="U3" pad="B5"/>
</signal>
<signal name="LIN9">
<contactref element="U2" pad="12"/>
<contactref element="U3" pad="A6"/>
</signal>
<signal name="LIN10">
<contactref element="U2" pad="13"/>
<contactref element="U3" pad="B6"/>
</signal>
<signal name="LIN11">
<contactref element="U2" pad="14"/>
<contactref element="U3" pad="A7"/>
</signal>
<signal name="LIN12">
<contactref element="U2" pad="15"/>
<contactref element="U3" pad="B7"/>
</signal>
<signal name="LIN13">
<contactref element="U2" pad="16"/>
<contactref element="U3" pad="A8"/>
</signal>
<signal name="LIN14">
<contactref element="U2" pad="18"/>
<contactref element="U3" pad="A9"/>
</signal>
<signal name="LIN15">
<contactref element="U2" pad="20"/>
<contactref element="U3" pad="A10"/>
</signal>
<signal name="LIN16">
<contactref element="U2" pad="21"/>
<contactref element="U3" pad="B10"/>
</signal>
<signal name="LIN17">
<contactref element="U2" pad="22"/>
<contactref element="U3" pad="A11"/>
</signal>
<signal name="LIN18">
<contactref element="U2" pad="23"/>
<contactref element="U3" pad="B11"/>
</signal>
<signal name="5V0">
<contactref element="C8" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="REG1" pad="3"/>
<contactref element="REG1" pad="5"/>
<contactref element="U1" pad="2"/>
<contactref element="POKEYMAX1" pad="17"/>
</signal>
<signal name="3V3">
<contactref element="U3" pad="B9"/>
<contactref element="U3" pad="D8"/>
<contactref element="U3" pad="H7"/>
<contactref element="U3" pad="G8"/>
<contactref element="U3" pad="F7"/>
<contactref element="U3" pad="G6"/>
<contactref element="U3" pad="G3"/>
<contactref element="U3" pad="C7"/>
<contactref element="U3" pad="G11"/>
<contactref element="U3" pad="K3"/>
<contactref element="U3" pad="C8"/>
<contactref element="U3" pad="F2"/>
<contactref element="U3" pad="J3"/>
<contactref element="U3" pad="J11"/>
<contactref element="U3" pad="H11"/>
<contactref element="U3" pad="C6"/>
<contactref element="U3" pad="F11"/>
<contactref element="U3" pad="E7"/>
<contactref element="FB1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U2" pad="17"/>
<contactref element="REG1" pad="6"/>
<contactref element="L1" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JTAG" pad="2"/>
<contactref element="REG2" pad="4"/>
<contactref element="REG2" pad="3"/>
<contactref element="U4" pad="17"/>
<contactref element="R6" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$137">
<contactref element="REG1" pad="2"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="TCK">
<contactref element="R3" pad="1"/>
<contactref element="U3" pad="G2"/>
<contactref element="JTAG" pad="4"/>
</signal>
<signal name="TDO">
<contactref element="U3" pad="F6"/>
<contactref element="JTAG" pad="6"/>
</signal>
<signal name="TMS">
<contactref element="U3" pad="G1"/>
<contactref element="R2" pad="1"/>
<contactref element="JTAG" pad="1"/>
</signal>
<signal name="TDI">
<contactref element="U3" pad="F5"/>
<contactref element="R1" pad="1"/>
<contactref element="JTAG" pad="3"/>
</signal>
<signal name="LIN19">
<contactref element="U2" pad="24"/>
<contactref element="U3" pad="A12"/>
</signal>
<signal name="LVLA18">
<contactref element="U2" pad="34"/>
<contactref element="POKEYMAX1" pad="35"/>
</signal>
<signal name="AUD1">
<contactref element="RN3" pad="8"/>
<contactref element="U3" pad="C10"/>
</signal>
<signal name="AUD3">
<contactref element="RN3" pad="5"/>
<contactref element="U3" pad="C9"/>
</signal>
<signal name="AUD4">
<contactref element="RN3" pad="6"/>
<contactref element="U3" pad="D9"/>
</signal>
<signal name="CONF_DONE">
<contactref element="U3" pad="C5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="3V3A">
<contactref element="U3" pad="K9"/>
<contactref element="U3" pad="D10"/>
<contactref element="U3" pad="D4"/>
<contactref element="U3" pad="K4"/>
<contactref element="FB1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="FAKE_CLK">
<contactref element="U3" pad="G9"/>
<contactref element="U3" pad="H8"/>
</signal>
<signal name="LVLA6">
<contactref element="U2" pad="47"/>
<contactref element="POKEYMAX1" pad="29"/>
</signal>
<signal name="LIN20">
<contactref element="U2" pad="25"/>
<contactref element="U3" pad="B12"/>
</signal>
<signal name="LIN21">
<contactref element="U2" pad="26"/>
<contactref element="U3" pad="B13"/>
</signal>
<signal name="LIN22">
<contactref element="U2" pad="27"/>
<contactref element="U3" pad="C12"/>
</signal>
<signal name="LIN23">
<contactref element="U2" pad="28"/>
<contactref element="U3" pad="D13"/>
</signal>
<signal name="LVLA21">
<contactref element="U2" pad="31"/>
<contactref element="AUD" pad="4"/>
</signal>
<signal name="LVLA19">
<contactref element="U2" pad="33"/>
<contactref element="POKEYMAX1" pad="26"/>
</signal>
<signal name="LVLA7">
<contactref element="U2" pad="46"/>
<contactref element="POKEYMAX1" pad="28"/>
</signal>
<signal name="AUDF1">
<contactref element="U1" pad="15"/>
<contactref element="RN2" pad="8"/>
<contactref element="POKEYMAX1" pad="37"/>
</signal>
<signal name="LVLA23">
<contactref element="U2" pad="29"/>
<contactref element="POKEYMAX1" pad="23"/>
</signal>
<signal name="NSTATUS">
<contactref element="U3" pad="C4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="LVLA13">
<contactref element="U2" pad="40"/>
<contactref element="POKEYMAX1" pad="36"/>
</signal>
<signal name="LVLA10">
<contactref element="U2" pad="43"/>
<contactref element="POKEYMAX1" pad="31"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="14"/>
<contactref element="C3" pad="1"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="AUDF2">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="AMPIN4P">
<contactref element="U1" pad="12"/>
<contactref element="CN1" pad="6"/>
<contactref element="RN3" pad="3"/>
</signal>
<signal name="AMPIN3P">
<contactref element="U1" pad="9"/>
<contactref element="CN1" pad="5"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="AMPIN1M">
<contactref element="U1" pad="16"/>
<contactref element="RN2" pad="1"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="AMPIN3M">
<contactref element="U1" pad="8"/>
<contactref element="RN2" pad="3"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="13"/>
<contactref element="RN1" pad="5"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="AMPIN1P">
<contactref element="CN1" pad="8"/>
<contactref element="RN3" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="ADC_RX">
<contactref element="R10" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="M13"/>
</signal>
<signal name="ADC_TX">
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="L11"/>
</signal>
<signal name="2V5">
<contactref element="U3" pad="L8"/>
<contactref element="U3" pad="L6"/>
<contactref element="U3" pad="L7"/>
<contactref element="REG2" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="RN2" pad="6"/>
</signal>
<signal name="LVLB0">
<contactref element="U4" pad="54"/>
<contactref element="POKEYMAX1" pad="22"/>
</signal>
<signal name="LVLB1">
<contactref element="U4" pad="53"/>
<contactref element="POKEYMAX1" pad="21"/>
</signal>
<signal name="LVLB2">
<contactref element="U4" pad="52"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="LVLB3">
<contactref element="U4" pad="51"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="LVLB5">
<contactref element="U4" pad="48"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="LVLB6">
<contactref element="U4" pad="47"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="LVLB7">
<contactref element="U4" pad="46"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="LVLB4">
<contactref element="U4" pad="50"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="NC1">
<contactref element="U3" pad="M11"/>
</signal>
<signal name="LVLB8">
<contactref element="U4" pad="45"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="LVLB9">
<contactref element="U4" pad="44"/>
<contactref element="C12" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="LVLB10">
<contactref element="U4" pad="43"/>
<contactref element="POKEYMAX1" pad="8"/>
</signal>
<signal name="LVLB11">
<contactref element="U4" pad="42"/>
<contactref element="POKEYMAX1" pad="9"/>
</signal>
<signal name="LVLB12">
<contactref element="U4" pad="41"/>
<contactref element="POKEYMAX1" pad="10"/>
</signal>
<signal name="LVLB13">
<contactref element="U4" pad="40"/>
<contactref element="POKEYMAX1" pad="11"/>
</signal>
<signal name="LVLB14">
<contactref element="U4" pad="39"/>
<contactref element="POKEYMAX1" pad="14"/>
</signal>
<signal name="LVLB15">
<contactref element="U4" pad="37"/>
<contactref element="POKEYMAX1" pad="15"/>
</signal>
<signal name="LVLB16">
<contactref element="U4" pad="36"/>
<contactref element="POKEYMAX1" pad="13"/>
</signal>
<signal name="LVLB17">
<contactref element="U4" pad="35"/>
<contactref element="POKEYMAX1" pad="12"/>
</signal>
<signal name="LVLB18">
<contactref element="U4" pad="34"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="LVLB19">
<contactref element="U4" pad="33"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="LVLB20">
<contactref element="U4" pad="32"/>
<contactref element="POKEYMAX1" pad="20"/>
</signal>
<signal name="LVLB21">
<contactref element="U4" pad="31"/>
<contactref element="POKEYMAX1" pad="19"/>
</signal>
<signal name="LVLB22">
<contactref element="U4" pad="30"/>
<contactref element="POKEYMAX1" pad="18"/>
</signal>
<signal name="LVLB23">
<contactref element="U4" pad="29"/>
<contactref element="POKEYMAX1" pad="16"/>
</signal>
<signal name="LINB0">
<contactref element="U4" pad="2"/>
<contactref element="U3" pad="G12"/>
</signal>
<signal name="LINB1">
<contactref element="U4" pad="3"/>
<contactref element="U3" pad="G13"/>
</signal>
<signal name="LINB2">
<contactref element="U4" pad="4"/>
<contactref element="U3" pad="H13"/>
</signal>
<signal name="LINB3">
<contactref element="U4" pad="5"/>
<contactref element="U3" pad="J12"/>
</signal>
<signal name="LINB4">
<contactref element="U4" pad="6"/>
<contactref element="U3" pad="J13"/>
</signal>
<signal name="LINB5">
<contactref element="U4" pad="7"/>
<contactref element="U3" pad="K13"/>
</signal>
<signal name="LINB6">
<contactref element="U4" pad="9"/>
<contactref element="U3" pad="L12"/>
</signal>
<signal name="LINB7">
<contactref element="U4" pad="10"/>
<contactref element="U3" pad="L13"/>
</signal>
<signal name="LINB8">
<contactref element="U4" pad="11"/>
<contactref element="U3" pad="K12"/>
</signal>
<signal name="LINB9">
<contactref element="U4" pad="12"/>
<contactref element="U3" pad="M12"/>
</signal>
<signal name="LINB10">
<contactref element="U4" pad="13"/>
<contactref element="U3" pad="L10"/>
</signal>
<signal name="LINB11">
<contactref element="U4" pad="14"/>
<contactref element="U3" pad="N9"/>
</signal>
<signal name="LINB12">
<contactref element="U4" pad="15"/>
<contactref element="U3" pad="M9"/>
</signal>
<signal name="LINB13">
<contactref element="U4" pad="16"/>
<contactref element="U3" pad="N8"/>
</signal>
<signal name="LINB14">
<contactref element="U4" pad="18"/>
<contactref element="U3" pad="M7"/>
</signal>
<signal name="LINB15">
<contactref element="U4" pad="20"/>
<contactref element="U3" pad="N5"/>
</signal>
<signal name="LINB16">
<contactref element="U4" pad="21"/>
<contactref element="U3" pad="M5"/>
</signal>
<signal name="LINB17">
<contactref element="U4" pad="22"/>
<contactref element="U3" pad="L4"/>
</signal>
<signal name="LINB18">
<contactref element="U4" pad="23"/>
<contactref element="U3" pad="L3"/>
</signal>
<signal name="LINB19">
<contactref element="U4" pad="24"/>
<contactref element="U3" pad="M3"/>
</signal>
<signal name="LINB20">
<contactref element="U4" pad="25"/>
<contactref element="U3" pad="M2"/>
</signal>
<signal name="LINB21">
<contactref element="U4" pad="26"/>
<contactref element="U3" pad="M1"/>
</signal>
<signal name="LINB22">
<contactref element="U4" pad="27"/>
<contactref element="U3" pad="L1"/>
</signal>
<signal name="LINB23">
<contactref element="U4" pad="28"/>
<contactref element="U3" pad="K1"/>
</signal>
<signal name="PTHRES">
<contactref element="U3" pad="M10"/>
<contactref element="U3" pad="N10"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="M8"/>
<contactref element="U3" pad="N7"/>
<contactref element="U3" pad="N6"/>
<contactref element="U3" pad="N4"/>
<contactref element="U3" pad="M4"/>
<contactref element="U3" pad="L5"/>
</signal>
<signal name="AUDF3">
<contactref element="C4" pad="2"/>
<contactref element="AUD" pad="3"/>
</signal>
<signal name="AUDF4">
<contactref element="AUD" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="AUD_IN">
<contactref element="C12" pad="2"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="OSC_CLOCK">
<contactref element="X1" pad="3"/>
<contactref element="U3" pad="F13"/>
<contactref element="U3" pad="E13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
